
Flank protection at junctions:

Lever    Requires              
-----    --------
 12     19 Normal
 13     24 Normal
 19     12 Normal
 24     13 Normal
 35     12 Reverse
 36     12 Reverse
 

Ground Shunt signals:

Lever    Applies to        Note
-----    ----------        ----
  8      Up Main           Requires Line Clear
  9      Up Rugby          Requires Line Clear
 10      Up Nuneaton       To signal 7
 17      Down Main         To signal 41
 29      (not in use)      See Local Information
 34      (not in use)      See Local Information
 41      Down Goods        To signal 49/50
 47      Headshunt         To buffer stops         
 49      Down Goods        To Limit of Shunt
 50      Down Yard

Other:

Fixed Distant signals are provided on the Down Goods and Up Goods line.

The Normal position of no.19 points is set towards the North Curve and the Normal position of no.24 points is set towards the Nuneaton line.

